Digital Multi-channel

Biocare ECG-8080 Tablet ECG Machine



Features

7 inches color LCD with grid line, display as printing

Touch-screen, input by hand writing for convenient operation

Unlimited SD card data storage with useful management tools

Unique acquisition technique, facilitate abnormal ECG acquisition

12+1 leads display and print out make observation easier

Real time waveform freezing, record any period of waveform by different format

Long life Li-ion battery for continuous operation

Wire or wireless data transmission, information management and sharing system

Multi-language versions available

Supports a USB laser printer

Includes a 2 year warranty

Biocare ECG-8080 Tablet Digital ECG Machine

Digital Multi-channel ECG

 